# Channel table for SãO MIGUEL DO IGUAçU-PR - Brazil
# Source: https://portalbsd.com.br/terrestres_channels.php?cidade=269

# Physical channel 26 (virtual 29.1)
[RIC tv Oeste]
	DELIVERY_SYSTEM = ISDBT
	BANDWIDTH_HZ = 6000000
	FREQUENCY = 545142857
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	ISDBT_LAYER_ENABLED = 7
	ISDBT_SOUND_BROADCASTING = 0
	ISDBT_SB_SUBCHANNEL_ID = 0
	ISDBT_SB_SEGMENT_IDX = 0
	ISDBT_SB_SEGMENT_COUNT = 0
	ISDBT_LAYERA_FEC = AUTO
	ISDBT_LAYERA_MODULATION = QAM/AUTO
	ISDBT_LAYERA_SEGMENT_COUNT = 0
	ISDBT_LAYERA_TIME_INTERLEAVING = 0
	ISDBT_LAYERB_FEC = AUTO
	ISDBT_LAYERB_MODULATION = QAM/AUTO
	ISDBT_LAYERB_SEGMENT_COUNT = 0
	ISDBT_LAYERB_TIME_INTERLEAVING = 0
	ISDBT_LAYERC_FEC = AUTO
	ISDBT_LAYERC_MODULATION = QAM/AUTO
	ISDBT_LAYERC_SEGMENT_COUNT = 0
	ISDBT_LAYERC_TIME_INTERLEAVING = 0

# Physical channel 28 (virtual 6.1)
[TV Tarobá Cascavel]
	DELIVERY_SYSTEM = ISDBT
	BANDWIDTH_HZ = 6000000
	FREQUENCY = 557142857
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	ISDBT_LAYER_ENABLED = 7
	ISDBT_SOUND_BROADCASTING = 0
	ISDBT_SB_SUBCHANNEL_ID = 0
	ISDBT_SB_SEGMENT_IDX = 0
	ISDBT_SB_SEGMENT_COUNT = 0
	ISDBT_LAYERA_FEC = AUTO
	ISDBT_LAYERA_MODULATION = QAM/AUTO
	ISDBT_LAYERA_SEGMENT_COUNT = 0
	ISDBT_LAYERA_TIME_INTERLEAVING = 0
	ISDBT_LAYERB_FEC = AUTO
	ISDBT_LAYERB_MODULATION = QAM/AUTO
	ISDBT_LAYERB_SEGMENT_COUNT = 0
	ISDBT_LAYERB_TIME_INTERLEAVING = 0
	ISDBT_LAYERC_FEC = AUTO
	ISDBT_LAYERC_MODULATION = QAM/AUTO
	ISDBT_LAYERC_SEGMENT_COUNT = 0
	ISDBT_LAYERC_TIME_INTERLEAVING = 0

# Physical channel 39 (virtual 12.1)
[Rede Massa Naipi]
	DELIVERY_SYSTEM = ISDBT
	BANDWIDTH_HZ = 6000000
	FREQUENCY = 623142857
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	ISDBT_LAYER_ENABLED = 7
	ISDBT_SOUND_BROADCASTING = 0
	ISDBT_SB_SUBCHANNEL_ID = 0
	ISDBT_SB_SEGMENT_IDX = 0
	ISDBT_SB_SEGMENT_COUNT = 0
	ISDBT_LAYERA_FEC = AUTO
	ISDBT_LAYERA_MODULATION = QAM/AUTO
	ISDBT_LAYERA_SEGMENT_COUNT = 0
	ISDBT_LAYERA_TIME_INTERLEAVING = 0
	ISDBT_LAYERB_FEC = AUTO
	ISDBT_LAYERB_MODULATION = QAM/AUTO
	ISDBT_LAYERB_SEGMENT_COUNT = 0
	ISDBT_LAYERB_TIME_INTERLEAVING = 0
	ISDBT_LAYERC_FEC = AUTO
	ISDBT_LAYERC_MODULATION = QAM/AUTO
	ISDBT_LAYERC_SEGMENT_COUNT = 0
	ISDBT_LAYERC_TIME_INTERLEAVING = 0

# Physical channel 41 (virtual 25.1)
[RPC Foz do Iguaçu]
	DELIVERY_SYSTEM = ISDBT
	BANDWIDTH_HZ = 6000000
	FREQUENCY = 635142857
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	ISDBT_LAYER_ENABLED = 7
	ISDBT_SOUND_BROADCASTING = 0
	ISDBT_SB_SUBCHANNEL_ID = 0
	ISDBT_SB_SEGMENT_IDX = 0
	ISDBT_SB_SEGMENT_COUNT = 0
	ISDBT_LAYERA_FEC = AUTO
	ISDBT_LAYERA_MODULATION = QAM/AUTO
	ISDBT_LAYERA_SEGMENT_COUNT = 0
	ISDBT_LAYERA_TIME_INTERLEAVING = 0
	ISDBT_LAYERB_FEC = AUTO
	ISDBT_LAYERB_MODULATION = QAM/AUTO
	ISDBT_LAYERB_SEGMENT_COUNT = 0
	ISDBT_LAYERB_TIME_INTERLEAVING = 0
	ISDBT_LAYERC_FEC = AUTO
	ISDBT_LAYERC_MODULATION = QAM/AUTO
	ISDBT_LAYERC_SEGMENT_COUNT = 0
	ISDBT_LAYERC_TIME_INTERLEAVING = 0

# Physical channel 43 (virtual 43.1)
[TV Novo Tempo]
	DELIVERY_SYSTEM = ISDBT
	BANDWIDTH_HZ = 6000000
	FREQUENCY = 647142857
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	ISDBT_LAYER_ENABLED = 7
	ISDBT_SOUND_BROADCASTING = 0
	ISDBT_SB_SUBCHANNEL_ID = 0
	ISDBT_SB_SEGMENT_IDX = 0
	ISDBT_SB_SEGMENT_COUNT = 0
	ISDBT_LAYERA_FEC = AUTO
	ISDBT_LAYERA_MODULATION = QAM/AUTO
	ISDBT_LAYERA_SEGMENT_COUNT = 0
	ISDBT_LAYERA_TIME_INTERLEAVING = 0
	ISDBT_LAYERB_FEC = AUTO
	ISDBT_LAYERB_MODULATION = QAM/AUTO
	ISDBT_LAYERB_SEGMENT_COUNT = 0
	ISDBT_LAYERB_TIME_INTERLEAVING = 0
	ISDBT_LAYERC_FEC = AUTO
	ISDBT_LAYERC_MODULATION = QAM/AUTO
	ISDBT_LAYERC_SEGMENT_COUNT = 0
	ISDBT_LAYERC_TIME_INTERLEAVING = 0

# Physical channel 50 (virtual 59.3)
[Rede Vida, Rede Vida +, Rede Vida Educação]
	DELIVERY_SYSTEM = ISDBT
	BANDWIDTH_HZ = 6000000
	FREQUENCY = 689142857
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	ISDBT_LAYER_ENABLED = 7
	ISDBT_SOUND_BROADCASTING = 0
	ISDBT_SB_SUBCHANNEL_ID = 0
	ISDBT_SB_SEGMENT_IDX = 0
	ISDBT_SB_SEGMENT_COUNT = 0
	ISDBT_LAYERA_FEC = AUTO
	ISDBT_LAYERA_MODULATION = QAM/AUTO
	ISDBT_LAYERA_SEGMENT_COUNT = 0
	ISDBT_LAYERA_TIME_INTERLEAVING = 0
	ISDBT_LAYERB_FEC = AUTO
	ISDBT_LAYERB_MODULATION = QAM/AUTO
	ISDBT_LAYERB_SEGMENT_COUNT = 0
	ISDBT_LAYERB_TIME_INTERLEAVING = 0
	ISDBT_LAYERC_FEC = AUTO
	ISDBT_LAYERC_MODULATION = QAM/AUTO
	ISDBT_LAYERC_SEGMENT_COUNT = 0
	ISDBT_LAYERC_TIME_INTERLEAVING = 0

