# Channel table for ChinaSat 6C at 130.5°E
# Source: http://www.lyngsat.com/ChinaSat-6C.html

[CCTV]
	DELIVERY_SYSTEM = DVBS
	FREQUENCY = 3860000
	POLARIZATION = VERTICAL
	SYMBOL_RATE = 26600000
	INNER_FEC = AUTO
	INVERSION = AUTO

