# Switzerland, Geneva region
# Updated by tkernen@deckpoint.ch on 2010/12/03
#------------------------------------------------------------------------------
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 570166000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 578000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 5/6
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 658166000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/8
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 666166000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 682166000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/8
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 706000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 1/2
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 746166000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/8
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 762000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 1/2
	CODE_RATE_LP = NONE
	MODULATION = QPSK
	TRANSMISSION_MODE = 2K
	GUARD_INTERVAL = 1/32
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 770166000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/8
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 794166000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/8
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 818166000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/8
	HIERARCHY = NONE
	INVERSION = AUTO

[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 850166000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/8
	HIERARCHY = NONE
	INVERSION = AUTO

