# Australia / Mackay (Mt Blackwood transmitters)
# aufreq=((UHF channel number)*8+306)

# ABC
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 212500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

# Seven Network
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 205500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/8
	HIERARCHY = NONE
	INVERSION = AUTO

# WIN Digital
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 578500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

# Southern Cross Ten
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 557500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

# SBS
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 536500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/8
	HIERARCHY = NONE
	INVERSION = AUTO

