# Channel table for NAZáRIA-PI - Brazil
# Source: https://portalbsd.com.br/terrestres_channels.php?cidade=1772

# Physical channel 20 (virtual 20.3)
[TV Jornal, Rádio Boa FM, Rádio Cocais FM]
	DELIVERY_SYSTEM = ISDBT
	BANDWIDTH_HZ = 6000000
	FREQUENCY = 509142857
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	ISDBT_LAYER_ENABLED = 7
	ISDBT_SOUND_BROADCASTING = 0
	ISDBT_SB_SUBCHANNEL_ID = 0
	ISDBT_SB_SEGMENT_IDX = 0
	ISDBT_SB_SEGMENT_COUNT = 0
	ISDBT_LAYERA_FEC = AUTO
	ISDBT_LAYERA_MODULATION = QAM/AUTO
	ISDBT_LAYERA_SEGMENT_COUNT = 0
	ISDBT_LAYERA_TIME_INTERLEAVING = 0
	ISDBT_LAYERB_FEC = AUTO
	ISDBT_LAYERB_MODULATION = QAM/AUTO
	ISDBT_LAYERB_SEGMENT_COUNT = 0
	ISDBT_LAYERB_TIME_INTERLEAVING = 0
	ISDBT_LAYERC_FEC = AUTO
	ISDBT_LAYERC_MODULATION = QAM/AUTO
	ISDBT_LAYERC_SEGMENT_COUNT = 0
	ISDBT_LAYERC_TIME_INTERLEAVING = 0

# Physical channel 22 (virtual 7.2)
[Rede Meio, Rádio Meio Norte FM]
	DELIVERY_SYSTEM = ISDBT
	BANDWIDTH_HZ = 6000000
	FREQUENCY = 521142857
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	ISDBT_LAYER_ENABLED = 7
	ISDBT_SOUND_BROADCASTING = 0
	ISDBT_SB_SUBCHANNEL_ID = 0
	ISDBT_SB_SEGMENT_IDX = 0
	ISDBT_SB_SEGMENT_COUNT = 0
	ISDBT_LAYERA_FEC = AUTO
	ISDBT_LAYERA_MODULATION = QAM/AUTO
	ISDBT_LAYERA_SEGMENT_COUNT = 0
	ISDBT_LAYERA_TIME_INTERLEAVING = 0
	ISDBT_LAYERB_FEC = AUTO
	ISDBT_LAYERB_MODULATION = QAM/AUTO
	ISDBT_LAYERB_SEGMENT_COUNT = 0
	ISDBT_LAYERB_TIME_INTERLEAVING = 0
	ISDBT_LAYERC_FEC = AUTO
	ISDBT_LAYERC_MODULATION = QAM/AUTO
	ISDBT_LAYERC_SEGMENT_COUNT = 0
	ISDBT_LAYERC_TIME_INTERLEAVING = 0

# Physical channel 24 (virtual 2.2)
[TV Antares, Rádio Antares]
	DELIVERY_SYSTEM = ISDBT
	BANDWIDTH_HZ = 6000000
	FREQUENCY = 533142857
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	ISDBT_LAYER_ENABLED = 7
	ISDBT_SOUND_BROADCASTING = 0
	ISDBT_SB_SUBCHANNEL_ID = 0
	ISDBT_SB_SEGMENT_IDX = 0
	ISDBT_SB_SEGMENT_COUNT = 0
	ISDBT_LAYERA_FEC = AUTO
	ISDBT_LAYERA_MODULATION = QAM/AUTO
	ISDBT_LAYERA_SEGMENT_COUNT = 0
	ISDBT_LAYERA_TIME_INTERLEAVING = 0
	ISDBT_LAYERB_FEC = AUTO
	ISDBT_LAYERB_MODULATION = QAM/AUTO
	ISDBT_LAYERB_SEGMENT_COUNT = 0
	ISDBT_LAYERB_TIME_INTERLEAVING = 0
	ISDBT_LAYERC_FEC = AUTO
	ISDBT_LAYERC_MODULATION = QAM/AUTO
	ISDBT_LAYERC_SEGMENT_COUNT = 0
	ISDBT_LAYERC_TIME_INTERLEAVING = 0

# Physical channel 26 (virtual 4.3)
[TV Clube, Educa Piauí, A Escola em Minha Casa]
	DELIVERY_SYSTEM = ISDBT
	BANDWIDTH_HZ = 6000000
	FREQUENCY = 545142857
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	ISDBT_LAYER_ENABLED = 7
	ISDBT_SOUND_BROADCASTING = 0
	ISDBT_SB_SUBCHANNEL_ID = 0
	ISDBT_SB_SEGMENT_IDX = 0
	ISDBT_SB_SEGMENT_COUNT = 0
	ISDBT_LAYERA_FEC = AUTO
	ISDBT_LAYERA_MODULATION = QAM/AUTO
	ISDBT_LAYERA_SEGMENT_COUNT = 0
	ISDBT_LAYERA_TIME_INTERLEAVING = 0
	ISDBT_LAYERB_FEC = AUTO
	ISDBT_LAYERB_MODULATION = QAM/AUTO
	ISDBT_LAYERB_SEGMENT_COUNT = 0
	ISDBT_LAYERB_TIME_INTERLEAVING = 0
	ISDBT_LAYERC_FEC = AUTO
	ISDBT_LAYERC_MODULATION = QAM/AUTO
	ISDBT_LAYERC_SEGMENT_COUNT = 0
	ISDBT_LAYERC_TIME_INTERLEAVING = 0

# Physical channel 28 (virtual 5.3)
[TV Cidade Verde, TV Cidade Verde 5.2, Rádio CVMAIS]
	DELIVERY_SYSTEM = ISDBT
	BANDWIDTH_HZ = 6000000
	FREQUENCY = 557142857
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	ISDBT_LAYER_ENABLED = 7
	ISDBT_SOUND_BROADCASTING = 0
	ISDBT_SB_SUBCHANNEL_ID = 0
	ISDBT_SB_SEGMENT_IDX = 0
	ISDBT_SB_SEGMENT_COUNT = 0
	ISDBT_LAYERA_FEC = AUTO
	ISDBT_LAYERA_MODULATION = QAM/AUTO
	ISDBT_LAYERA_SEGMENT_COUNT = 0
	ISDBT_LAYERA_TIME_INTERLEAVING = 0
	ISDBT_LAYERB_FEC = AUTO
	ISDBT_LAYERB_MODULATION = QAM/AUTO
	ISDBT_LAYERB_SEGMENT_COUNT = 0
	ISDBT_LAYERB_TIME_INTERLEAVING = 0
	ISDBT_LAYERC_FEC = AUTO
	ISDBT_LAYERC_MODULATION = QAM/AUTO
	ISDBT_LAYERC_SEGMENT_COUNT = 0
	ISDBT_LAYERC_TIME_INTERLEAVING = 0

# Physical channel 31 (virtual 32.1)
[RFTV]
	DELIVERY_SYSTEM = ISDBT
	BANDWIDTH_HZ = 6000000
	FREQUENCY = 575142857
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	ISDBT_LAYER_ENABLED = 7
	ISDBT_SOUND_BROADCASTING = 0
	ISDBT_SB_SUBCHANNEL_ID = 0
	ISDBT_SB_SEGMENT_IDX = 0
	ISDBT_SB_SEGMENT_COUNT = 0
	ISDBT_LAYERA_FEC = AUTO
	ISDBT_LAYERA_MODULATION = QAM/AUTO
	ISDBT_LAYERA_SEGMENT_COUNT = 0
	ISDBT_LAYERA_TIME_INTERLEAVING = 0
	ISDBT_LAYERB_FEC = AUTO
	ISDBT_LAYERB_MODULATION = QAM/AUTO
	ISDBT_LAYERB_SEGMENT_COUNT = 0
	ISDBT_LAYERB_TIME_INTERLEAVING = 0
	ISDBT_LAYERC_FEC = AUTO
	ISDBT_LAYERC_MODULATION = QAM/AUTO
	ISDBT_LAYERC_SEGMENT_COUNT = 0
	ISDBT_LAYERC_TIME_INTERLEAVING = 0

# Physical channel 34 (virtual 10.3)
[TV Antena 10, A10+, A10+]
	DELIVERY_SYSTEM = ISDBT
	BANDWIDTH_HZ = 6000000
	FREQUENCY = 593142857
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	INVERSION = AUTO
	GUARD_INTERVAL = AUTO
	TRANSMISSION_MODE = AUTO
	ISDBT_LAYER_ENABLED = 7
	ISDBT_SOUND_BROADCASTING = 0
	ISDBT_SB_SUBCHANNEL_ID = 0
	ISDBT_SB_SEGMENT_IDX = 0
	ISDBT_SB_SEGMENT_COUNT = 0
	ISDBT_LAYERA_FEC = AUTO
	ISDBT_LAYERA_MODULATION = QAM/AUTO
	ISDBT_LAYERA_SEGMENT_COUNT = 0
	ISDBT_LAYERA_TIME_INTERLEAVING = 0
	ISDBT_LAYERB_FEC = AUTO
	ISDBT_LAYERB_MODULATION = QAM/AUTO
	ISDBT_LAYERB_SEGMENT_COUNT = 0
	ISDBT_LAYERB_TIME_INTERLEAVING = 0
	ISDBT_LAYERC_FEC = AUTO
	ISDBT_LAYERC_MODULATION = QAM/AUTO
	ISDBT_LAYERC_SEGMENT_COUNT = 0
	ISDBT_LAYERC_TIME_INTERLEAVING = 0

