# Channel table for SES 22 at 139.0°W
# Source: http://www.lyngsat.com/SES-22.html

[Alaskan mux]
	DELIVERY_SYSTEM = DVBS
	FREQUENCY = 4056000
	POLARIZATION = HORIZONTAL
	SYMBOL_RATE = 13250000
	INNER_FEC = AUTO
	INVERSION = AUTO

