# Channel table for SES 3 at 103.0°W
# Source: http://www.lyngsat.com/SES-3.html

[NTA International]
	DELIVERY_SYSTEM = DVBS2
	FREQUENCY = 12080000
	POLARIZATION = HORIZONTAL
	SYMBOL_RATE = 29970000
	MODULATION = PSK/8
	INNER_FEC = AUTO
	INVERSION = AUTO

