# DVB-T Baden-Württemberg
# Created from http://www.ueberallfernsehen.de/data/senderliste.pdf
[CH21: ZDF, 3sat, KiKa / ZDFneo, ZDFinfo]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 474000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH22: ZDF, 3sat, KiKa / ZDFneo, ZDFinfo]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 482000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH23: ZDF, 3sat, KiKa / ZDFneo, ZDFinfo]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 490000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH26: Das Erste, arte, Phoenix, EinsPlus]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 514000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH33: ZDF, 3sat, KiKa / ZDFneo, ZDFinfo]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 570000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH39: SWR-BW, Bayerisches Fernsehen, hr, WDR]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 618000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH40: SWR-BW, Bayerisches Fernsehen, hr, WDR]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 626000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH41: SWR-BW, Bayerisches Fernsehen, hr, WDR]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 634000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH43: Das Erste, arte, Phoenix, EinsPlus]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 650000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH45: RTL, RTL2, Super RTL, VOX, RTL Crime, Passion [Sendenorm: MPEG-4]]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 666000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/8
	HIERARCHY = NONE
	INVERSION = AUTO

[CH49: SWR-BW, Bayerisches Fernsehen, hr, WDR]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 698000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH50: SWR-BW, Bayerisches Fernsehen, hr, WDR]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 706000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH52: Das Erste, arte, Phoenix, EinsPlus]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 722000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH54: Das Erste, arte, Phoenix, EinsPlus]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 738000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH59: Das Erste, arte, Phoenix, EinsPlus]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 778000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH60: Das Erste, arte, Phoenix, EinsPlus]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 786000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

