# DVB-T Malaga (Andalucia)                   by Pedro Leon 4 Mayo 2007
[C57 La Primera, La 2, Canal 24H, Clan/TVE 50, RNE1, RNE Clásica, RNE 3]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 762000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C63 Canal Sur, Canal 2 Andalucia]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 810000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C66 TELEDEPORTE, VEO, *Canal Ingenieria, SETenVEO, Tienda en VEO, NET TV, Radio Intereconomia]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 834000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C67 CUATRO, CNN+, 40 LATINO, laSexta]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 842000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C68 Telecinco, T5 Estrellas, T5 Sport, FLYMUSIC, PUNTO RADIO]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 850000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[C69 ANTENA 3, ANTENA.NEOX, ANTENA.NOVA, *tvtv DIGITAL, ONDA CERO, EUROPA FM, ONDA MELODIA, Telehit]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 858000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

