# US NTSC center frequencies
# primarily of historical interest, many of these channels are no longer used
#
# see also: us-ATSC-center-frequencies-8VSB

#
# VHF low-band, channels 2 to 6, not used for digital
#

[CHANNEL 2]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 57028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 3]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 63028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 4]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 69028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 5]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 79028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 6]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 85028615
	MODULATION = VSB/8
	INVERSION = AUTO

#
# VHF high-band, channels 7 to 13. not common but a few digital stations use it
# potentially hard to receive because modern antennas are tuned for UHF
#

[CHANNEL 7]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 177028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 8]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 183028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 9]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 189028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 10]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 195028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 11]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 201028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 12]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 207028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 13]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 213028615
	MODULATION = VSB/8
	INVERSION = AUTO

#
# UHF, channels 14 to 51, most existing stations, almost all digital
#

[CHANNEL 14]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 473028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 15]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 479028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 16]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 485028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 17]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 491028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 18]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 497028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 19]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 503028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 20]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 509028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 21]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 515028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 22]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 521028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 23]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 527028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 24]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 533028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 25]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 539028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 26]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 545028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 27]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 551028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 28]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 557028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 29]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 563028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 30]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 569028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 31]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 575028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 32]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 581028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 33]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 587028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 34]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 593028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 35]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 599028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 36]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 605028615
	MODULATION = VSB/8
	INVERSION = AUTO

#channel 37, not used in North America due to interference with radio astronomy bands
[CHANNEL 37]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 611028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 38]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 617028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 39]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 623028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 40]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 629028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 41]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 635028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 42]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 641028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 43]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 647028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 44]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 653028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 45]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 659028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 46]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 665028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 47]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 671028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 48]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 677028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 49]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 683028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 50]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 689028615
	MODULATION = VSB/8
	INVERSION = AUTO

#
# the following frequencies were formerly part of the UHF band before the digital transition
# but were sold off to cell carriers in 2010 as the 700 MHz band and are no longer used for television
#

#channel 51 was originally included in the digital transition but
# no longer used to clear interference with 700 MHz cell bands
[CHANNEL 51]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 695028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 52]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 701028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 53]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 707028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 54]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 713028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 55]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 719028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 56]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 725028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 57]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 731028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 58]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 737028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 59]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 743028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 60]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 749028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 61]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 755028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 62]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 761028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 63]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 767028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 64]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 773028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 65]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 779028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 66]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 785028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 67]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 791028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 68]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 797028615
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 69]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 803028615
	MODULATION = VSB/8
	INVERSION = AUTO

# UHF formerly had channels 70 through 83 as well

[CHANNEL 70]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 809000000
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 71]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 815000000
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 72]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 821000000
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 73]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 827000000
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 74]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 833000000
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 75]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 839000000
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 76]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 845000000
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 77]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 851000000
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 78]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 857000000
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 79]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 863000000
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 80]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 869000000
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 81]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 875000000
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 82]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 881000000
	MODULATION = VSB/8
	INVERSION = AUTO

[CHANNEL 83]
	DELIVERY_SYSTEM = ATSC
	FREQUENCY = 887000000
	MODULATION = VSB/8
	INVERSION = AUTO

