# Australia / Newcastle
# SBS
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 599500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/8
	HIERARCHY = NONE
	INVERSION = AUTO

# NBN
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 585500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

# Prime
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 578500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

# ABC
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 592500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

# SC10
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 606500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

