# DVB-T Nordrhein-Westfalen
# Created from http://www.ueberallfernsehen.de/data/senderliste.pdf
[CH25: WDR-Dortmund, NDR/WDR-Ruhr, MDR, SWR]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 506000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/8
	HIERARCHY = NONE
	INVERSION = AUTO

[CH26: Das Erste, arte, Phoenix, EinsFestival]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 514000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

                                            # CH26: ZDF, 3sat, KiKa / ZDFneo, ZDFinfo
[CH27: WDR-Südwestfalen, NDR, MDR, SWR]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 522000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 1/2
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH29: RTL, RTL2, Super RTL, VOX]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 538000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH30: ZDF, 3sat, KiKa / ZDFneo, ZDFinfo]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 546000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH31: WDR-OWL_aktuell, NDR/WDR-Südwestfalen, MDR, SWR]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 554000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 1/2
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH33: ZDF, 3sat, KiKa / ZDFneo, ZDFinfo]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 570000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH35: ZDF, 3sat, KiKa / ZDFneo, ZDFinfo]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 586000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH36: Tele5, CNN, Eurosport, VIVA]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 594000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH37: WDR-Aachen, NDR/WDR-Köln, MDR, SWR]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 602000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 1/2
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH46: WDR-Düsseldorf, MDR/WDR-Duisburg, NDR/WDR-Berg.Land, SWR]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 674000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 1/2
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH48: Das Erste, arte, Phoenix, EinsFestival]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 690000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH49: WDR-Köln, MDR/WDR-Bonn, NDR/WDR-Aachen, SWR]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 698000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 1/2
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH50: Das Erste, arte, Phoenix, EinsFestival]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 706000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH52: Tele5, CNN, Eurosport, VIVA]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 722000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH53: ProSieben, Sat.1, Kabel1, N24]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 730000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH55: ProSieben, Sat.1, Kabel1, N24]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 746000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

[CH57: WDR-Ruhr, NDR/WDR-Dortmund, MDR, SWR]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 762000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/8
	HIERARCHY = NONE
	INVERSION = AUTO

[CH60: Das Erste, arte, Phoenix, EinsFestival]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 786000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = 2/3
	CODE_RATE_LP = NONE
	MODULATION = QAM/16
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/4
	HIERARCHY = NONE
	INVERSION = AUTO

