# Lithuania, whole country
# Created from http://www.skaitmenine.lt/lt/skaitmenine_tv_lietuvoje/antzemine_dvb_t.html
# Created by baruse@gmail.com

# LRTC I tinklas
[kanalas 22]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 482000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

[kanalas 26]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 514000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

[kanalas 39]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 618000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

[kanalas 44]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 658000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

[kanalas 47]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 682000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

[kanalas 57]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 762000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

[kanalas 58]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 770000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

[kanalas 60]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 786000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

[kanalas 61]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 794000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO


# LRTC II tinklas
[kanalas 33]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 570000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

[kanalas 38]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 610000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

[kanalas 48]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 690000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

[kanalas 54]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 738000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

[kanalas 62]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 802000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

[kanalas 63]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 810000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

[kanalas 64]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 818000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO


# TEO LT I tinklas
[kanalas 36]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 594000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

[kanalas 50]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 706000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

[kanalas 59]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 778000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

[kanalas 65]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 826000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO


# TEO LT II tinklas
[kanalas 21]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 474000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

[kanalas 30]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 546000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

[kanalas 53]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 730000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

#T 786000000 8MHz AUTO NONE QAM64 8k 1/16 NONE # kanalas 60

# Vilniui bonusas
[kanalas 37]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 602000000
	BANDWIDTH_HZ = 8000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

