# Australia / Goulburn / Rocky Hill
#
# Scanned 31/07/2016 - Alex Ferrara (alex@receptiveit.com.au)

[Nine Canberra]
	SERVICE_ID = 2055
	VIDEO_PID = 353
	AUDIO_PID = 354
	PID_0b = 8026
	PID_06 = 355
	PID_05 = 8025
	FREQUENCY = 641500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[9HD Canberra]
	SERVICE_ID = 2247
	VIDEO_PID = 1761
	AUDIO_PID = 1762 1763 8025
	PID_0b = 8026
	FREQUENCY = 641500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[Nine Canberra]
	SERVICE_ID = 2215
	VIDEO_PID = 353
	AUDIO_PID = 354
	PID_0b = 8026
	PID_06 = 355
	PID_05 = 8025
	FREQUENCY = 641500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[9Gem]
	SERVICE_ID = 2087
	VIDEO_PID = 1711
	AUDIO_PID = 1712
	PID_0b = 8026
	PID_06 = 1713
	PID_05 = 8025
	FREQUENCY = 641500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[9Go!]
	SERVICE_ID = 2119
	VIDEO_PID = 1721
	AUDIO_PID = 1722
	PID_0b = 8026
	PID_06 = 1723
	PID_05 = 8025
	FREQUENCY = 641500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[9Life]
	SERVICE_ID = 2279
	VIDEO_PID = 1771
	AUDIO_PID = 1772
	PID_0b = 8026
	PID_06 = 1773
	PID_05 = 8025
	FREQUENCY = 641500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[YESSHOP]
	SERVICE_ID = 2151
	VIDEO_PID = 1731
	AUDIO_PID = 1732
	PID_0b = 8026
	PID_05 = 8025
	FREQUENCY = 641500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[Aspire]
	SERVICE_ID = 2183
	VIDEO_PID = 1741
	AUDIO_PID = 1742
	PID_0b = 8026
	PID_05 = 8025
	FREQUENCY = 641500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[WIN Canberra]
	SERVICE_ID = 1921
	VIDEO_PID = 122
	AUDIO_PID = 522
	PID_0b = 102
	PID_06 = 722
	FREQUENCY = 634500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[WIN Canberra HD]
	SERVICE_ID = 1939
	VIDEO_PID = 125
	AUDIO_PID = 525 725
	PID_0b = 102
	FREQUENCY = 634500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[ONE Canberra]
	SERVICE_ID = 1922
	VIDEO_PID = 123
	AUDIO_PID = 523
	PID_0b = 102
	PID_06 = 723
	FREQUENCY = 634500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[ELEVEN Canberra]
	SERVICE_ID = 1926
	VIDEO_PID = 124
	AUDIO_PID = 524
	PID_0b = 102
	PID_06 = 724
	FREQUENCY = 634500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[WIN NETWORK]
	SERVICE_ID = 1936
	VIDEO_PID = 126
	AUDIO_PID = 526
	PID_0b = 102
	PID_06 = 726
	FREQUENCY = 634500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[TVSN]
	SERVICE_ID = 1928
	VIDEO_PID = 116
	AUDIO_PID = 516
	PID_0b = 102
	PID_06 = 716
	FREQUENCY = 634500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[GOLD]
	SERVICE_ID = 1927
	VIDEO_PID = 115
	AUDIO_PID = 515
	PID_0b = 102
	PID_06 = 715
	FREQUENCY = 634500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[ONE Canberra]
	SERVICE_ID = 1925
	VIDEO_PID = 123
	AUDIO_PID = 523
	PID_0b = 102
	PID_06 = 723
	FREQUENCY = 634500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[WIN Canberra]
	SERVICE_ID = 1924
	VIDEO_PID = 122
	AUDIO_PID = 522
	PID_0b = 102
	PID_06 = 722
	FREQUENCY = 634500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[PRIME7 Canberra]
	SERVICE_ID = 2374
	VIDEO_PID = 2740
	AUDIO_PID = 2741
	PID_0b = 2749
	PID_06 = 2745
	FREQUENCY = 627500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[PRIME7 Canberra]
	SERVICE_ID = 2400
	VIDEO_PID = 2740
	AUDIO_PID = 2741
	PID_0b = 2749
	PID_06 = 2745
	FREQUENCY = 627500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[PRIME7 Canberra]
	SERVICE_ID = 2401
	VIDEO_PID = 2740
	AUDIO_PID = 2741
	PID_0b = 2749
	PID_06 = 2745
	FREQUENCY = 627500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[7TWO Canberra]
	SERVICE_ID = 2402
	VIDEO_PID = 4620
	AUDIO_PID = 4621
	PID_0b = 2749
	PID_06 = 4625
	FREQUENCY = 627500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[7mate Canberra]
	SERVICE_ID = 2403
	VIDEO_PID = 4630
	AUDIO_PID = 4632 4635
	PID_0b = 2749
	FREQUENCY = 627500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[ishoptv]
	SERVICE_ID = 2405
	VIDEO_PID = 4650
	AUDIO_PID = 4651
	PID_0b = 2749
	FREQUENCY = 627500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[RACING.COM]
	SERVICE_ID = 2408
	VIDEO_PID = 4680
	AUDIO_PID = 4681
	PID_0b = 2749
	FREQUENCY = 627500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[ABC News 24]
	SERVICE_ID = 672
	VIDEO_PID = 516
	AUDIO_PID = 654 580 5500
	PID_0b = 5501 5000
	FREQUENCY = 620500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[ABC]
	SERVICE_ID = 673
	VIDEO_PID = 512
	AUDIO_PID = 650
	PID_0b = 5501 5000
	PID_06 = 576
	PID_05 = 5500
	FREQUENCY = 620500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[ABC2/KIDS]
	SERVICE_ID = 674
	VIDEO_PID = 513
	AUDIO_PID = 651
	PID_0b = 5501 5000
	PID_06 = 577
	PID_05 = 5500
	FREQUENCY = 620500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[ABC]
	SERVICE_ID = 675
	VIDEO_PID = 512
	AUDIO_PID = 650
	PID_0b = 5501 5000
	PID_06 = 576
	PID_05 = 5500
	FREQUENCY = 620500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[ABC3]
	SERVICE_ID = 676
	VIDEO_PID = 514
	AUDIO_PID = 652
	PID_0b = 5501 5000
	PID_06 = 578
	PID_05 = 5500
	FREQUENCY = 620500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[Double J]
	SERVICE_ID = 678
	AUDIO_PID = 690
	PID_0b = 5501
	PID_05 = 5500
	FREQUENCY = 620500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[ABC Jazz]
	SERVICE_ID = 679
	AUDIO_PID = 700
	PID_0b = 5501
	PID_05 = 5500
	FREQUENCY = 620500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[SBS ONE]
	SERVICE_ID = 849
	VIDEO_PID = 161
	AUDIO_PID = 81
	PID_0b = 7000 5000
	PID_06 = 41
	PID_05 = 7849
	FREQUENCY = 613500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[SBS HD]
	SERVICE_ID = 853
	VIDEO_PID = 102
	AUDIO_PID = 103
	PID_0b = 7000 5000
	PID_06 = 43
	PID_05 = 7853
	FREQUENCY = 613500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[SBS TWO]
	SERVICE_ID = 850
	VIDEO_PID = 162
	AUDIO_PID = 83
	PID_0b = 7000 5000
	PID_06 = 42
	PID_05 = 7850
	FREQUENCY = 613500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[Food Network]
	SERVICE_ID = 851
	VIDEO_PID = 163
	AUDIO_PID = 85
	PID_0b = 7000 5000
	PID_06 = 44
	PID_05 = 7849
	FREQUENCY = 613500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[NITV]
	SERVICE_ID = 852
	VIDEO_PID = 164
	AUDIO_PID = 87
	PID_0b = 7000 5000
	PID_06 = 45
	PID_05 = 7852
	FREQUENCY = 613500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[SBS Radio 1]
	SERVICE_ID = 862
	AUDIO_PID = 201
	FREQUENCY = 613500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[SBS Radio 2]
	SERVICE_ID = 863
	AUDIO_PID = 202
	FREQUENCY = 613500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

[SBS Radio 3]
	SERVICE_ID = 864
	AUDIO_PID = 203
	FREQUENCY = 613500000
	MODULATION = QAM/256
	BANDWIDTH_HZ = 0
	INVERSION = AUTO
	CODE_RATE_HP = NONE
	CODE_RATE_LP = AUTO
	GUARD_INTERVAL = 1/32
	TRANSMISSION_MODE = 2K
	HIERARCHY = NONE
	DELIVERY_SYSTEM = DVBT

