# Australia / Melbourne (Selby Repeater)
# ABC
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 662500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

# Seven
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 620500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

# Nine
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 641500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

# Ten
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 711500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = 3/4
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/16
	HIERARCHY = NONE
	INVERSION = AUTO

# SBS
[CHANNEL]
	DELIVERY_SYSTEM = DVBT
	FREQUENCY = 683500000
	BANDWIDTH_HZ = 7000000
	CODE_RATE_HP = AUTO
	CODE_RATE_LP = NONE
	MODULATION = QAM/64
	TRANSMISSION_MODE = 8K
	GUARD_INTERVAL = 1/8
	HIERARCHY = NONE
	INVERSION = AUTO

